“Whisper” Winterizing
Date:

1 Purchase
___1.1 Antifreeze: 14 gal -60( & 4 gal -100(
___1.2 Oil: Rotella-T SAE 15W-40 [8 qts]

___1.3 Filter: NAPA 1515 or Wix 51515
___1.4 Motor antifreeze: Frostfree LS ethylene glycol

2 Exterior
___2.1 Pump-out

___2.2 Remove sails

___2.3 Remove covers

___2.4 Remove screens

___2.5 Stow/clean dingy

___2.6 Remove dingy engine 
(___self-service or ___yard)
___2.7 Remove davits (7/16 wrench & Phillips)
___2.8 Remove motor lift

___2.9 Remove ring buoy

___2.10 Remove EPIRB (take home)
___2.11 Remove exterior compass (home)
___2.12 Remove BBQ grill

___2.13 Remove seats & dry cushions (7/16 socket)

___2.14 Lower GPS antenna (5/16 hex)

___2.15 Loosen shrouds/stays (looking down – turn clockwise) – ½” wrench & large screwdriver
___2.15.1 Remove screws (9/32 socket & Phillips screwdriver)

___2.15.2 Front shrouds: 4 half turns

___2.15.3 Middle shrouds: 6 half turns 
___2.15.4 Back shrouds: 2 half turns
___2.15.5 Rear stay: 6 half turns

___2.16 Stow water hose

___2.17 Secure lines

3 Dingy engine

___3.1 Fog

___3.2 Remove gas

___3.3 Oil crankcase

___3.4 Change sparkplug

4 Engine (in water)

___4.1 Log engine hours

___4.2 Run engine to operating temperature (190oF)
___4.3 Drain oil

___4.4 Change filter (turn counter-clockwise)

___4.5 Add oil (start @ 7 qts & use all 8)

___4.6 Check antifreeze to ____ [-34(]
___4.7 Change fuel filters

___4.7.1 Primary: _______ (yearly)

___4.7.2 Secondary: ________ (10/23/05)
___4.8 Wipe down engine bilge

___4.9 Check alternator belt

___4.10 Check raw water impellor

___4.11 Grease pillow block

___4.12 Fill water in batteries (distilled)
5 Fuel

___5.1 Top off tanks, if needed (____ gal each)
Fuel remaining _____ gal each
___5.2 Biocide (1 oz/30 gal)
6 Westabo heater

___6.1 Change fuel filter

___6.2 Check antifreeze to -34°

7 Air Conditioning (1.5 gal antifreeze)
___7.1 Close thru-hull

___7.2 Rinse condenser (cockpit)

___7.3 Clean & stow filter (with washer)

___7.4 Install filter-hose attachment
___7.5 Blowout pump (bilge)
___7.6 Open AC shut-off

___7.7 Blowout condenser (cockpit)
___7.8 Replace filter cover
___7.9 Antifreeze pump [1 gal]
___7.10 Close AC shut-off

___7.11 Antifreeze condenser (use funnel) [0.5 gal]
___7.12 Remove filter cover

___7.13 Spray down rear bilge

8 Washdown pump (0.5 gal antifreeze)
___8.1 Remove hose

___8.2 Open spigot

___8.3 Drain line (5/16 socket)
___8.4 Antifreeze pump [0.5 gal]

___8.5 Clean & stow filter (no washer) – use channel locks
___8.6 Spray down front bilge

9 Waste/head (3 gal antifreeze)
___9.1 Flush head lines

___9.2 Flush tank twice

___9.3 Flush macerator

___9.4 Empty tank

___9.5 Antifreeze intake lines & conditioner [5/16 socket for clamp) [0.5 gal]

___9.6 Antifreeze tank – from pump-out [1 gal]

___9.7 Antifreeze head – pump through lines [1.5 gal] 

___9.8 Antifreeze macerator (run pump 10 sec)

10 Shower pump (before dingy stowage)
___10.1 Run shower pump
___10.2 Antifreeze line & pump [0.5 gal]

___10.3 Clean & stow filter (no washer) – use channel locks
11 Frig

___11.1 Shut down

___11.2 Clean

12 Water (5.0 gal antifreeze)
___12.1 Turn off water heater breaker (tape)

___12.2 Shut off & drain water purifier

___12.3 Drain tanks

___12.4 Drain water heater (5/16 socket)
___12.5 Bypass water heater

___12.6 Blowout lines

___12.7 Empty galley faucet/spray and head faucet/shower valve

___12.8 Drain water purifier & reinstall
___12.9 Antifreeze hand/foot pumps [0.75 gal]

___12.10 Antifreeze lines [2 gal
___12.11 Antifreeze galley faucet/spray
___12.12 Antifreeze head faucet/shower valve

___12.13 Clean & stow pump filter – use channel locks
___12.14 Antifreeze tanks [2 gal each]
13 Interior

___13.1 Remove binoculars

___13.2 Remove first aid kits
___13.3 Remove batteries (nav table)
___13.4 Remove work freezables: under interior helm, under nav table, under qtr berth
___13.5 Remove food freezables (galley)
___13.6 Remove head freezables: medicine, suntan lotion, distilled water, etc.

___13.7 Stow rugs & blankets

___13.8 Remove computer, if needed
___13.9 Pack up files as needed

14 Propane

___14.1 Shut-off tanks

___14.2 Disconnect

MOVE TO WELL

15 Out of water (3 gal antifreeze)
___15.1 Connect shore power

___15.2 Charge batteries

___15.3 Open seacocks

___15.4 Bilge
___15.4.1 Drain (remove/reinsert garboard plug – plug handle in key drawer)

___15.4.2 Pump dry with hand pump
(pump handle in cockpit locker)
___15.4.3 Antifreeze electric bilge pump [2 gal]
___15.4.4 Antifreeze hand bilge pump (cockpit) [1 gal] - pump dry

___15.5 Galley seawater pump

___15.5.1 Pump dry

___15.5.2 Antifreeze from outside [0.25 gal]
(use 7’-0” ¼” ID black tubing)
___15.6 Remove garboard plug
___15.7 Engine raw water [2¾ gal of -100(]

___15.7.1 Run out water first

___15.7.2 Fill strainer & cap [0.25 gal]
___15.8 Stow rugs

___15.9 Power

___15.9.1 Turn off panel breakers
___15.9.2 Turn off engine compartment breakers

___15.9.3 Turn off Battery Parallel Switch

___15.9.4 Turn off Eng Bat Charge Switch

___15.9.5 Turn off Master

___15.9.6 Disconnect bank of 4 house batteries– check & disconnect (use 9/16 wrench)
___15.9.7 Disconnect bank of 2 starting batteries – check & disconnect (use small adjustable wrench)

___15.9.8 Disconnect shore power and stow cord

___15.10 Exterior

___15.10.1 Close blower & heater exhaust vents

___15.10.2 Stow fenders

___15.10.3 Stow dock lines

___15.10.4 Secure halyards

___15.10.5 Touch-up varnish

___15.11 Clean cockpit scuppers & cockpit
___15.12 Lock cockpit lockers

___15.13 Secure whisker pole

___15.14 Shrink wrap (yard)

16 Spring

___16.1 Fill propane tanks

___16.2 Wash exterior screens

17 Questions

___17.1 Cutlass bearing inlet?

___17.2 Engine exhaust wet vent?
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