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1981 BABA 35

Builder: TaShing

Designer: Robert Perry

LOA: 39'00" Approx Incl. Bowsprit

LOD: 34'11"; LWL: 29'08"

BEAM: 11'02"; DRAFT: 5'06"

DISPL: 22,000; BALLAST 7600  

MAST HT: Approx 55ft.

RIG: Cutter; SAIL AREA 716 sq. ft.

AUX: Perkins 44 hp 4-108; FUEL 55 gal; WATER 100 gal.

Sleeps 5

This vessel began its life in Maine where it saw use (approximately 12-15 years) primarily during the summers and was stored under cover during the winter.  The present owner is the third owner.  The vessel is in excellent shape and a survey is available to interested buyers.  The second owner very extensively outfitted the vessel for a circumnavigation.  This involved, among many, many items: total rebuild of engine and transmission by AKR Marine with a Dual RACOR 500 filter system; all new rigging, electrical, galley systems, new tanks, Lectra-San, water maker, bedding, etc., etc. etc.

The vessel’s construction exceed Lloyds specifications; single piece molded hand-laid solid fiberglass hull and deck with teak.  The deck is bonded and fastened to hull with stainless steel thru-bolts.  There is a raised teak bulwark with stainless steel cap, rub rail with stainless steel cap, full keep with internal cast iron ingot ballast.  Spars are aluminum and the mast keel-stepped.  Pedestal mounted wheel steering with cable and quadrant.  The rudder is mounted on keep.  Apeture in keel and rudder protects propeller.

INTERIOR APPOINTMENTS
6'04" headroom with superb varnished teak joinery throughout.  Voluminous storage, seven Apenglo high output/low draw 12v cabin lights with red light.  Generous open bronze ports.

FORWARD CABIN
A spacious V berth sleeps two comfortable on special custom 6" hinged foam mattress (‘97).  Custom fitted sheets.  Storage beneath berth.  Lexan overhead hatch.  Louvered door access to the chain locker.  Three opening ports and two Hella fans assist in ventilation.  There is, in addition, a private door to the head, copious drawer storage, shelves, and a large cedar-lined locker for clothes storage.

HEAD
Located to port immediate aft of forward cabin, the head offers a vanity with single stainless steel sink and marble counter top, water pressure, a Wilcox Crittenden Skipper marine toilet (‘93), Lectr-San treatment system, Y-valve for direct discharge, and very generous storage for linens etc.

MAIN SALON
Straight settees port and starboard, all with custom cushions.  There is a beautiful centerline drop-leaf table with inserts below and exquisite butterfly hatch that brings loads of light and air into the salon. Custom cabinets, copious storage, a Dickenson Newport heater and brass trawler lamp round out the salon that sleeps two and can easily accommodate six for dinner.

GALLEY
Located to port at the foot of the companionway, the galley offers a wonderful new Broadwater four-burner stove with oven and broiler; twin polished stainless steel sinks, and a superb Glacier Bay 12v refrigerator.  Additional items include: water pressure plus fresh and saltwater pumps, microwave, varnished teak and holly counters, and enough storage for a family of four on an extended voyage.

NAV STATION
Located to the starboard at the foot of the companionway, facing forward, the station has a large lift top chart table with storage, large instrument array panel, electric distribution panel, shelving and lockers.

QUARTER BERTH
This berth is located to the starboard at the foot of the companionway and accommodates 6'0" plus sailor.

AUXILIARY DIESEL
Spectacular engine access under companionway, with box-type cover removed without tools.  Astoundingly clean Perkins 44hp, 4 cyl, FWC, totally rebuilt engine and transmission by AKR marine in 2001, including new liners, tappets, pistons, valves and guides, cam shaft oil pump, injectors, and heat exchanger.  New prop shaft, dampening plate, dripless shaft seal, and hoses.  3 blade Michigan RH 18x10 prop, with spare.  Specially designed dual RACOR 500 series filter system always instant switch to new filter.  All fuel has been run through a Baha filter.  Algae-X system.

TANKAGE
Two new baffled diesel tanks (34 gal. forward, 21 gal. aft) mounted on DriDek to keep tanks out of bilge area.  Two baffled 50 gal. stainless steel water tanks under settees.  Forty gallon holding tank.

PLUMBING
Pressure water, stainless steal distribution manifold, filtration system, Power Survivor 35 watermaker. Lectra-San treatment system.  Manual and electric bildge pumps plus extra.  All new Groco bronze thru-hill etc. in ‘97.

ELECTRICAL
110vAC and 12v DC electrical systems.  New  gel batteries.  110v-12v distribution panels with master and individual circuit breakers; 125v shore power receptacle.  106 amp Ample Power engine alternator.  External Ample Power multi-stage regulator; Heart Freedom 10 (1000 watt) inverter-charger (50 amp).  Ample Power eliminator separates engine battery start battery from house bank during charging.  Ample Power Energy Monitor II for 12v system.  All very heavy-duty wiring, new.  High grade, large capacity grounding system for all metals, including mast, through large keel mounted copper discharge plate.

NAVIGATION
Pedastal mounted Ritchie compass; Standard Horizon Intrepid GX 1260S VHF at nave station with full function control remote microphone at helm; West Marine Kona VHF; 40 channel CB; portable radio.  Autohelm ST50 at help and at nav. desk; Autohelm 6000 autopilot; Sitex T180 Radar; Magellan 5200 GPS and differential, plus hand-held Magellan GPS and spares.  New Garmin GPS/Chartplotter plus charts; The Capn. w/extensive electronic charts.  Many paper charts plus books.  Orion TV/VCR.

GROUND TACKLE
Two 35# CQR with 200 5/16" HT chain plus additional chain for emergency conditions.  Simpson Lawrence Pacific Series V-1500 electric windlass.  Spare anchors, rode, snubber etc.

SPARS, RIGGING AND WINCHES
Aluminum mast and boom, stainless steel strand rigging, Pro-Furl roller furling for job and staysail.  Total of nine Barient winches, all self-tailing.  Total of three sails.

COCKPIT
Weblon dodger and Bimini in outstanding condition and provides wonderful protection.  Davits for dinghy.

ADDITIONAL
Caribe 9ft hard bottom inflatable dinghy and 9.9 OB.  Lots of fenders, fender boards, new dock lines, new Magma grill, emergency tiller.  Read starboard cockpit locker for 2 propane tanks and regulator, plus custom hose for direct connection to grill which allows simultaneous operation of grill and stove.  It would take many pages to list extras, spare parts that accompany this finely-appointed boat.  The boat is ready to take you anywhere in the world you want to go.

Asking price: $83, 500

Contact: Clifton Crais at ccrais@emory.edu
Serious inquires only, please.

