Baba 30

Agnes Lee

The Agnes Lee is the perfect boat for 2 people.  She is a Robert Perry design built in 1980 by TaShing, one of the best boat builders in Taiwan.  She is a fiberglass boat with teak decks and a full keel.  She was commissioned in 1981 and is a double-ended cutter that is a true off shore vessel. She has beautiful lines and a design that makes her safe, dry and extremely seaworthy. If you’re looking for a live aboard or you’re ready to take that extended voyage, then this is the boat for you.
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Specifications:
LOA: 29', 9"
LWL: 24' 6"
Beam 10' 3"
Displacement: approx 12,500
Full keel, 4' 9" draft
6' 3" headroom
Cream-colored hull
Forespar aluminum spars
Wheel steering 
Price - $60,000
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Layout
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Main saloon, port & starboard seating, storage behind & above
Fixed, folding leaf table 
Butterfly hatch in main saloon
Dickinson Newport solid fuel cabin heater

Spacious upper bilge for storage
Spacious double berth
Large hatch over berth
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Brass lamps, ship’s clock and barometer included.
Wet hanging locker
Navigation table
Lee cloths on both settees
10 port lights total; (3 in berth area)
2 cowl vents on Dorade boxes
Head with combined wash basin/shower
1 large, deep cockpit locker

Sails/Winches: 

Main with two reef points
Yankee
Staysail
130 genoa
Profurl on head stay

Lazy Jacks on main
Sail covers and ready bags
Jiffy Reefing, outhaul, and topping lift
Cockpit Winches


(2) Barient #23, self-tailing


(2) Barient #10P


(1) Barient main sheet winch, self-tailing

Mast Winches


(2) Barient #10


(1) Barient #10P

Galley:
Well-insulated, top-loading ice box
Sail Mate propane 2-burner stove with oven
Electric/engine heat exchanger hot water heater
Double stainless sink with covers

Pressurized hot and cold water

Bronze hand pump

Foot pump

Ample storage

All kitchen equipment and utensils are included
Electrical/Electronics:
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Standard Horizon VHF radio

Stowe depth sounder

Stowe speed and distance log

Ritchie Globemaster binnacle compass

Garmin 50 GPS

Stowe wind speed indicator

Adequate lights and signals for type and use

AM/FM/tape
12-volt and 110-volt electric
(2) 12-volt DC, deep cycle batteries equipped 

   with battery combiner

Shore power cord
Professional Mariner 3-bank battery charger

Auxiliary propulsion:
Yanmar 3-GM30F diesel engine installed by Palmer Johnson in 1995  Low usage

Fresh water cooled
Tankage/pumps:
Water – (2) 40 gallon stainless tanks under each settee

Fuel – Approximately 30 gallon, modified steel covered with epoxy

Holding – Approximately 30 gallon

Bilge pumps – 1 manual and 1 12 volt electric

Ground tackle:
25# CQR anchor w/70’ chain and 150’ rode 

12# Danforth anchor w/15’ chain and 150’ rode

Miscellaneous:

Double windlass with gypsies
Teak bow sprit with teak platform

Sampson post
Stainless steel, double-tiered bow and stern pulpits

Stainless steel stanchions with double life lines 
   with boarding gates to starboard and port. 

Custom made stainless moveable boarding ladder

Cockpit dodger with grab bars
Cockpit awing

Force 10 propane grill

9 ft. inflatable West Marine dinghy with 3.3 hp Mercury outboard 2000
All specifications are accurate to the best of owner’s knowledge.
Bill Jordan/Donna Knicely


5024 Patterson Ave.


Richmond, VA 23226
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